BTECH DA-7X2 V1.05d2 — STANDARD
================================

Use this folder for normal DMR and analog operation when NXDN is not
intentionally configured.

Keep the .spi, .CDI, and .CDD files together. In the CPS firmware updater,
select only DMR-7X2_V1.05d2_20260805.spi from this folder.

Do not combine these files with the NXDN folder.

Follow 08_GUIDES/DA-7X2_V1.05_Firmware_Update_Guide.pdf.
