BTECH DA-7X2 V1.05 UPDATE PACKAGE
=================================

This package is for the BTECH DA-7X2 only.

START HERE

1. Open 00_START_HERE_DA-7X2_V1.05.pdf.
2. Read 01_RELEASE_NOTES_DA-7X2_V1.05.pdf.
3. With your currently working BTECH CPS, read the radio and save a
   codeplug backup. Close and reopen it, then store a second copy elsewhere.
4. Install CPS V1.05d from 03_CPS_V1.05d.
5. Choose one firmware folder:
   - 04_FIRMWARE_STANDARD_RECOMMENDED for DMR and analog use.
   - 05_FIRMWARE_NXDN when you intentionally use NXDN.
6. Follow 08_GUIDES/DA-7X2_V1.05_Firmware_Update_Guide.pdf.
7. Reset the radio with PTT + PF1, restore the codeplug, and read it back.
8. Confirm firmware V1.05d2 and verify your settings before transmitting.

If VFO mode or expected menu items are missing, use
08_GUIDES/DA-7X2_Initial_Setup_Guide.pdf.

IMPORTANT

The Standard and NXDN folders contain identically named .spi, .CDI, and .CDD
files. Keep each triplet together. Select only the .spi file inside the one
firmware folder you chose. Never mix the two variants.

Support: https://baofengtech.com/support/
Email: support@baofengtech.com
