BTECH DA-7X2 CPS V1.05d
=======================

Before installing:
1. Use the currently working BTECH CPS to read the radio.
2. Save the codeplug with the model and date in the filename.
3. Close and reopen the backup.
4. Store a second copy on another device or trusted cloud location.

Then run DA_7X2_Setup_1.05d.exe.

Use the detailed migration guide in 08_GUIDES if you are restoring a saved
codeplug after the firmware reset.
